Lab 1

LED practical

Code:

void setup()

{

pinMode(13, OUTPUT);

}

void loop()

{

digitalWrite(13, HIGH);

delay(1000); // Wait for 1000 millisecond(s)

digitalWrite(13, LOW);

delay(1000); // Wait for 1000 millisecond(s)

}

Demonstration:



